C	av00	01-mar-02	First compile with Gnu77 compiler for windows
C				(Thanks to Raymond Anderson for letting me know
C				about this compiler and doing initial compilations)
C	av01	14-mar-02	Var PI not used in routine GWAVE
C	av02	14-mar-02	Sub SECOND already intrinsic function
C	av03	15-mar-02	SOMNEC routines integrated into Nec2D.exe
C	av04	16-mar-02	Status='NEW', does not seem to replace existing file.
C	av05	21-okt-02	Max number of loads (LOADMX) made equal to max-nr segments.
C	av06	21-okt-02	Max number of NT cards (NETMX) increased from 3O to (param)
C	av07	21-okt-02	Max number of EX cards (NSMAX) increased from 30 to (param)
C	av08	22-oct-02	Use of VSRC is uncertain, in some sources equal 10 and some
C				equal 30 (=nr EX?).  
C	av10	30-jan-03	Used DJGPP port of G77 compiler which delivers speed increase
C				from 30 to 60% for small segment counts
C	av11	04-sep-03	Logging of NetMX, NSMAX changed.
C	av12	29-sep-03	Enable user-specified NGF file-name.
C	av13	29-sep-03	MinGW port used for both 11K segs and virtual memory usage.
C	av14	09-oct-03	Max-nr of segs at junction/single-seg (JMAX) from 30 to 60.
