             The NEC-2D program is used to compute the YGO-optimized
     Yagi's electrical performance.  Because run time depends on how
     many segments are used, YGO includes several different versions
     of NEC-2D to allow a wide range of model sizes.  The NEC execut-
     able files are compressed into self-extracting EXE files.  To
     recover a specific version, run the extraction file in your
     default directory.  Be sure enough disk space is available, and
     that your system has enough RAM to execute both the NEC program
     and YGO.EXE at the same time.  The table below provides details.

     RUNNING THIS FILE....RECOVERS >>>>>> THIS FILE
     Self-Extracting                      ---------       Uncompressed
         EXE File      Max Segments    NEC-2D File Name   Size (bytes)
     ---------------   ------------    ----------------   ------------
       NSE_0028.EXE         28            NEC2D28.EXE         558,572
       NSE_0100.EXE        100           NEC2D100.EXE         733,388
       NSE_0250.EXE        250           NEC2D250.EXE       1,630,380 
       NSE_0500.EXE        500           NEC2D500.EXE       4,725,388
       NSE_0750.EXE        750           NEC2D750.EXE       9,820,380
       NSE_1100.EXE       1100            N2D1100.EXE      20,313,388
